Mechanical Problems:

The Wobble in the robot is due to following reasons:

1) Bearing Wobbling



2) Weaker Mounting with the stand



3) Weaker Cantilever Part Design

